

**Monitor Host Upgrade Guide**

**June 01 2009**

**0.1**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Revision** | **Description** | **Author** |
| June 01 2009 | 0.1 | Document Baseline | Cristian Guef |
| August 31 2009 | 0.3 | Every upgrader kit (from 14.1.08 ver.) will be divided in 2 parts: one for Full ISA Interface and one for Simple ISA Interface | Cristian Guef |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Table of Contents**

[1 Introduction 4](#_Toc235530785)

[1.1 Document Purpose 4](#_Toc235530786)

[1.2 Audience 4](#_Toc235530787)

[1.3 Abbreviations and Acronyms 4](#_Toc235530788)

[2 Upgrade steps 4](#_Toc235530789)

# Introduction

## Document Purpose

This document describes the necessary steps involved in upgrading Monitor Host application.

## Audience

Intended audience – the users installing/running Monitor Host application.

## Abbreviations and Acronyms

MH –Monitor Host application

DB -database

# Upgrade steps

The following steps are required to upgrade the MH:

1. Use a browser to connect to Admin Web Interface at URL http://<MiniPC IP>/MonitorHostAdmin/ and log in using username = “admin” and password = “!admin”.
2. Choose SYSTEM UPGRADE from menu, upload the archive file and click Save. A log with the installation progress will be displayed on the page.
3. To test the installation, check it Monitor Host application is running, by accessing the URL http://<MiniPC IP>/MonitorHostSite/ and also use a Terminal to check the running processes. Please give several minutes to the network to reform.